NVRAM Files Will Be Stored Here.

(N V R A M = Non-Volatile Random Access Memory)

NVRAMs Contain The Internal Settings Of The ROMs.

They Will Be Created Automatically When You Start A Table For The First Time.



NVRAM NOTE 1 - EARLY SOLID-STATE WILLIAMS TABLES:
-------------------------------------------------
Early Solid-State WILLIAMS Tables Have To Be Started A SECOND TIME In Order
To Become Functional Because The Very First Start Will Only Set The Machine To
Its Factory-Defaults First! (And Create The NVRAM In This Case.)
This Behaviour Is Normal, Its The Same As On The Real Machines When The NVRAM
Is Empty Due To Power Loss After Say A Battery Change.
So If Any Early WILLIAMS Solid-State Table Only Shows Its Production Number
In The Player1 Display, And Nothing Seems To Happen, Press F3 To Restart The ROM
And The Table Will Become Operational Right Away.




NVRAM NOTE 2 - Existing NVRAMs In This Folder:
----------------------------------------------
The NVRAMs For Some Tables (Mostly GOTTLIEB and BALLY Games) Are Already
Present In This Folder Because These Tables Will Not Accept Coins When Their
NVRAM Is Created Anew. This Behaviour Is Normal, Its The Same As On The Real
Machines When The NVRAM Is Empty Due To Power Loss After Say A Battery Change.
Unlike The Aforementioned WILLIAMS These Machines Have To Be TOTALLY Re-Configured
After A NVRAM Power Loss, And Since This Is Rather Complicated The NVRAMs For
These Machines Are Already Included In The VIP For Your Convenience.